Task

 Hazard

 Analysis

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Customer: |  | Job #: |  | Date: |  |
| City, State: |  | Foreman: |  | Time: |  |
| Description of work: |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Temp & Conditions: | Start: |  | End: |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Yes | No |  | Yes | No |  |
|[ ] [ ]  Hard hat, safety glasses, gloves, ear protection |[ ] [ ]  Hi-viz vest |
|[ ] [ ]  Fall protection inspected-harness & lanyard  |[ ] [ ]  Guards on all power tools |
|[ ] [ ]  Face shield welding hood |[ ] [ ]  GFCI outlet or GFCI Pig tail for electric cords |
|[ ] [ ]  Respirator |[ ] [ ]  Manlift, forklift – If yes, inspect and document |
|[ ] [ ]  Inspect rigging |[ ] [ ]  Barricades |
|[ ] [ ]  Chain fall inspected |[ ] [ ]  LOTO |

|  |
| --- |
| [ ]  Hot work / [ ]  Grinding / [ ]  Cutting / [ ]  Welding / [ ]  Open Flame (select one) |
| List hot work start time:  |  | End time: |  |
| List special precautions: |  |
| Yes | No |  |
|[ ] [ ]  Fire extinguisher within 10ft. of hot work |
|[ ] [ ]  Other trades on job site notified of hot work and duration |
|[ ] [ ]  Fire watch List name: |
|[ ] [ ]  Final check after completion of hot work  | *Client Policy:* |  | *List time:* |  |

|  |
| --- |
| Jobsite: Get your crew together – Take 5 minutes to assess the job |
| Look for and discuss obvious hazards and LIST HERE: | Mitigation (how will we handle it): |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  |  | *Post Task* | *Stretch & Flex* |  |  | *Post Task* | *Stretch & Flex* |
| Foreman: |  |  |  | Other: |  |  |  |
| Other: |  |  |  | Other: |  |  |  |
| Other: |  |  |  | Other: |  |  |  |
| Other: |  |  |  | Other: |  |  |  |
|  |  |  |  |  |  |  |  |
| Field Superintendent Sign: |  | *Post Task* |  | *Stretch & Flex* |  |